**Cisco 6509 Switch**

***Global Configuration:***

ip wccp version 2 [Version of WCCP]

ip wccp 0 password mypass (Optional) [Should match service group password in WCG (0=port 80)]

ip wccp 70 password mypass (Optional) [Should match service group password in WCG (0=port 443)]

ip wccp 0 redirect-list 10 [ACL applied to service group 0]

ip wccp 70 redirect-list 10 [ACL applied to service group 70]

***Interface Configuration:***

interface Vlan 36 [Internet facing Vlan]

ip wccp 0 redirect out [redirects outbound port 80 traffic to WCG web cache]

ip wccp 70 redirect out [redirects outbound port 443 traffic to WCG web cache]

***Access List 10:***

permit 10.20.69.199 [ACL permitting host 10.20.69.199 to WCG web cache]

permit 10.20.39.207 [ACL permitting host 10.20.39.209 to WCG web cache]

permit 10.20.39.0 0.0.0.255 [ACL permitting network 10.20.39.0/24 to WCG web cache]

**Warning :**

“you need https decryption enabled and functioning before redirecting https traffic to the V10000 using WCCP”

